(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 1)
    (tracks 46)
    (zones 0)
    (modules 10)
    (nets 6)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 V+)
  (net 2 GND)
  (net 3 "Net-(IC1-Pad3)")
  (net 4 "Net-(IC1-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad3)")
    (add_net V+)
  )
  (module ML_2AA_Eagle:SOT23-5 (layer Top) (tedit 0)
    (at 144.3101 105.8926 90)
    (fp_text reference IC1 (at -1.7272 0.9398) (layer F.SilkS))
    (fp_text value CAT4137 (at 3.048 1.778) (layer F.Fab))
    (pad 3 smd rect (at 0.95 1.306 90) (size 0.6 1.2) (layers Top F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0 1.306 90) (size 0.6 1.2) (layers Top F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.95 1.306 90) (size 0.6 1.2) (layers Top F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad1)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 0.95 -1.306 90) (size 0.6 1.2) (layers Top F.Paste F.Mask)
      (net 1 V+) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -0.95 -1.306 90) (size 0.6 1.2) (layers Top F.Paste F.Mask)
      (net 1 V+) (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:C0805 (layer Top) (tedit 0)
    (at 144.6911 102.5906 180)
    (fp_text reference C1 (at -1.3208 2.6416) (layer F.SilkS))
    (fp_text value 1uF (at -1.27 2.54) (layer F.Fab))
    (pad 2 smd rect (at 0.8499 0 180) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 1 V+) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.8499 0 180) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:C0805 (layer Top) (tedit 0)
    (at 153.4541 103.9876 270)
    (fp_text reference C2 (at -2.1082 1.8796) (layer F.SilkS))
    (fp_text value 220nF (at -1.27 2.54 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8499 0 270) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.8499 0 270) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:R0805 (layer Top) (tedit 0)
    (at 147.9931 100.4316)
    (descr "<b>RESISTOR</b><p>\nchip")
    (fp_text reference R1 (at -0.762 -1.016) (layer F.SilkS))
    (fp_text value 12 (at -0.762 2.286) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:LED5MM (layer Bottom) (tedit 0)
    (at 148.5011 105.0036 180)
    (descr "<B>LED</B><p>\n5 mm, round")
    (fp_text reference LED1 (at -2.54 3.4798) (layer B.SilkS))
    (fp_text value LED3MM (at 3.2004 -1.8034) (layer B.Fab) hide)
    (pad K thru_hole circle (at 1.27 0 180) (size 1.27 1.27) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad3)") (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at -1.27 0 180) (size 1.27 1.27) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:1X01 (layer Top) (tedit 0)
    (at 148.5011 106.0196)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference PIN_1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PINHD-1X1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4224 1.4224) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 V+) (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:1X01 (layer Top) (tedit 0)
    (at 148.5011 103.9876)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference PIN_2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PINHD-1X1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4224 1.4224) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:SOD-523F (layer Top) (tedit 0)
    (at 153.2001 107.7976 270)
    (fp_text reference D1 (at -1.4478 -0.7366 90) (layer F.SilkS))
    (fp_text value BAT54SOD-523F (at -2.54 2.54 90) (layer F.SilkS))
    (pad P$2 smd rect (at 1 0 90) (size 0.8 0.5) (layers Top F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad1)") (solder_mask_margin 0.1016))
    (pad P$1 smd rect (at -1 0 270) (size 0.8 0.5) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:05 (layer Top) (tedit 0)
    (at 146.6723 108.1278 90)
    (descr <b>JUMPER</b>)
    (fp_text reference J1 (at -2.119469 -1.006104 90) (layer F.SilkS))
    (fp_text value J5MM (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4224 1.4224) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.54 -0.0254 90) (size 1.4224 1.4224) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module ML_2AA_Eagle:COIL_CRAFT_ME3220_SERIES (layer Top) (tedit 0)
    (at 149.8981 108.7374)
    (descr "Surface mount inductor")
    (fp_text reference L1 (at 0.7366 -1.9558) (layer F.SilkS))
    (fp_text value 22uH (at -2.54 3.81) (layer F.Fab))
    (pad P$2 smd rect (at 1.143 0 90) (size 3.048 1.524) (layers Top F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad1)") (solder_mask_margin 0.1016))
    (pad P$1 smd rect (at -1.143 0.0254 90) (size 3.048 1.524) (layers Top F.Paste F.Mask)
      (net 1 V+) (solder_mask_margin 0.1016))
  )
  (gr_circle (center 148.5011 105.0036) (end 155.8671 105.0036) (layer Edge.Cuts) (width 0.127))
)
