<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="56.82" y2="0" width="0" layer="20"></wire>
<wire x1="56.82" y1="0" x2="56.82" y2="53.33" width="0" layer="20"></wire>
<wire x1="56.82" y1="53.33" x2="0" y2="53.33" width="0" layer="20"></wire>
<wire x1="0" y1="53.33" x2="0" y2="0" width="0" layer="20"></wire>
</plain>
<libraries>
<library name="AUTODESK_CIRCUITS_BREADBOARD">
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="RADIAL-D11.36MM">
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="SW2-12.7-12.0X3.6X3.6MM">
</package>
<package name="D-7.5">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="B25V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="C5B2.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 2.5 mm, grid 5.08 mm</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;5 mm, round</description>
</package>
<package name="LED-RGB-THRU">
</package>
<package name="PT-10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="TL1105">
<description>&lt;b&gt;TACT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://dkc3.digikey.com/Media/PDF/Data%20Sheets/E-Switch%20PDFs/TL1105%20Series.pdf</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
</package>
<package name="DC-POWER">
</package>
<package name="2P-2.54-65/35MIL">
</package>
<package name="1X3P-2.54-2.54-11.6-3.0-BLACK-MALE">
</package>
<package name="1X04">
</package>
<package name="1X05">
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X8P-2.54-2.54-11.6-3.0-BLACK-MALE">
</package>
<package name="1X9P-2.54-2.54-11.6-3.0-BLACK-MALE">
</package>
<package name="1X16P-2.54-2.54-11.6-3.0-BLACK-MALE">
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X4P-2.54-65/35MIL">
</package>
<package name="CR2032H">
<description>&lt;b&gt;LI BATTERY&lt;/b&gt; Varta</description>
</package>
<package name="M251">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor Buerklin, 11G702</description>
</package>
<package name="DIP02YL-DPST">
<description>&lt;b&gt;DIL/CODE SWITCH DPST&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="DIP04YL">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="DIP06YL">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="M3XXH">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
</package>
<package name="G6A-234P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
</package>
<package name="PIEZO-12MM">
</package>
<package name="PIEZO-22MM">
</package>
<package name="PHOTORESISTOR-2.54">
</package>
<package name="SNR6-D19.0MM">
</package>
<package name="7-SEGMENT-CC">
<description>&lt;b&gt;LED DISPLAY&lt;/b&gt;&lt;p&gt;
15-mm 1 character 7 segment, decimal point right</description>
</package>
<package name="HDSP-M">
<description>&lt;b&gt;LED DISPLAY&lt;/b&gt;&lt;p&gt;
15-mm 1 character 7 segment, decimal point right</description>
</package>
<package name="ARDUINO_UNO">
<description>Footprint for representing an Arduino Uno board in an EAGLE schematic.</description>
</package>
<package name="ARDUINO_MICRO">
<description>Footprint for representing an Arduino Micro board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element value="" name="U1" library="AUTODESK_CIRCUITS_BREADBOARD" package="ARDUINO_UNO"></element><element value="" name="SERVO1" library="AUTODESK_CIRCUITS_BREADBOARD" package="1X3P-2.54-2.54-11.6-3.0-BLACK-MALE"></element><element value="1k‎Ω" name="R1" library="AUTODESK_CIRCUITS_BREADBOARD" package="0207/10"></element><element value="" name="D1" library="AUTODESK_CIRCUITS_BREADBOARD" package="LED5MM"></element><element value="" name="D2" library="AUTODESK_CIRCUITS_BREADBOARD" package="LED5MM"></element><element value="1k‎Ω" name="R2" library="AUTODESK_CIRCUITS_BREADBOARD" package="0207/10"></element></elements>
<signals>
<signal name="N$1"><contactref element="U1" pad="9"></contactref><contactref element="SERVO1" pad="3"></contactref></signal><signal name="N$2"><contactref element="U1" pad="5V"></contactref><contactref element="SERVO1" pad="2"></contactref></signal><signal name="N$3"><contactref element="U1" pad="GND.."></contactref><contactref element="SERVO1" pad="1"></contactref></signal><signal name="N$4"><contactref element="U1" pad="2"></contactref><contactref element="R1" pad="1"></contactref></signal><signal name="N$5"><contactref element="R1" pad="2"></contactref><contactref element="D1" pad="K"></contactref></signal><signal name="N$6"><contactref element="U1" pad="3"></contactref><contactref element="R2" pad="1"></contactref></signal><signal name="N$7"><contactref element="R2" pad="2"></contactref><contactref element="D2" pad="K"></contactref><contactref element="D1" pad="A"></contactref><contactref element="U1" pad="GND."></contactref></signal><signal name="N$8"><contactref element="D2" pad="A"></contactref></signal></signals>
</board>
</drawing>
</eagle>