<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="55.9943" y1="92.075" x2="55.9943" y2="0.635" width="0.0254" layer="20" curve="186.762115"/>
<wire x1="55.9943" y1="92.075" x2="55.9943" y2="81.153" width="0.0254" layer="20"/>
<wire x1="55.9943" y1="81.153" x2="46.4185" y2="81.153" width="0.0254" layer="20"/>
<wire x1="46.4185" y1="81.153" x2="46.4185" y2="10.8204" width="0.0254" layer="20"/>
<wire x1="46.4185" y1="10.8204" x2="55.9943" y2="10.8204" width="0.0254" layer="20"/>
<wire x1="55.9943" y1="10.8204" x2="55.9943" y2="0.635" width="0.0254" layer="20"/>
<text>Inspired by</text>
<text>Nikolai Kikitin &amp; NSL</text>
<text>GND</text>
<text>5V</text>
<text>19x16=304 Blinkies!</text>
<text>SUPPLY</text>
<text>Rev. C</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP15SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="thecustomgeek">
<description>A humble collection of custom parts.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="atmel-1">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="WS8212B Clear Thru-Hole">
<packages>
<package name="HDRV4W64P254_1X4_1016X508X838B">
<description>Single-row, 4-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 10.16 X 5.08 X 8.38 mm body
&lt;p&gt;Single-row (1X4), 4-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with overall size 10.16 X 5.08 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="V3_slice_noshift">
<description>Generated from &lt;b&gt;V3_slice_noshift.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA07-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V" library="testpad" package="TP15SQ" value="TPTP15SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="testpad" package="TP15SQ" value="TPTP15SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="IN" library="testpad" package="TP15SQ" value="TPTP15SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="testpad" package="TP15SQ" value="TPTP15SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="thecustomgeek" package="TQFP32-08" value="ATMEGA328"/>
<element name="Q1" library="crystal" package="HC49/S" value="16MHz"/>
<element name="C20" library="adafruit" package="C1206" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C21" library="adafruit" package="C1206" value="22pF">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R1206" value="10K">
<attribute name="NAME"/>
</element>
<element name="C22" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="atmel-1" package="AVR-ISP-6" value="AVR-ISP-6">
<attribute name="NAME"/>
</element>
<element name="SUPPLY" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D2" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D3" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D4" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D5" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D6" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D7" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D8" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D9" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D10" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D11" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D12" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D13" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D14" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D15" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D16" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D17" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D18" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="D19" library="WS8212B Clear Thru-Hole" package="HDRV4W64P254_1X4_1016X508X838B" value="WS8212B-C-THRU-HOLE">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V1" library="testpad" package="TP15SQ" value="TPTP15SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="GNDIN" library="testpad" package="TP15SQ" value="TPTP15SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C1206" value="220uF">
<attribute name="NAME"/>
</element>
<element name="10K2" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SEQ_BUTTON" library="V3_slice_noshift" package="TACTILE-PTH" value=""/>
<element name="ACCEL" library="con-lstb" package="MA07-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="4"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GND" pad="TP"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="C22" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="SUPPLY" pad="1"/>
<contactref element="D1" pad="3"/>
<contactref element="D2" pad="3"/>
<contactref element="D3" pad="3"/>
<contactref element="D4" pad="3"/>
<contactref element="D5" pad="3"/>
<contactref element="D6" pad="3"/>
<contactref element="D7" pad="3"/>
<contactref element="D8" pad="3"/>
<contactref element="D9" pad="3"/>
<contactref element="D10" pad="3"/>
<contactref element="D11" pad="3"/>
<contactref element="D12" pad="3"/>
<contactref element="D13" pad="3"/>
<contactref element="D14" pad="3"/>
<contactref element="D15" pad="3"/>
<contactref element="D16" pad="3"/>
<contactref element="D17" pad="3"/>
<contactref element="D18" pad="3"/>
<contactref element="D19" pad="3"/>
<contactref element="GNDIN" pad="TP"/>
<contactref element="C1" pad="1"/>
<contactref element="10K2" pad="2"/>
<contactref element="ACCEL" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="5V" pad="TP"/>
<contactref element="SUPPLY" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="D11" pad="2"/>
<contactref element="D12" pad="2"/>
<contactref element="D13" pad="2"/>
<contactref element="D14" pad="2"/>
<contactref element="D15" pad="2"/>
<contactref element="D16" pad="2"/>
<contactref element="D17" pad="2"/>
<contactref element="D18" pad="2"/>
<contactref element="D19" pad="2"/>
<contactref element="5V1" pad="TP"/>
<contactref element="C1" pad="2"/>
<contactref element="SEQ_BUTTON" pad="2"/>
<contactref element="ACCEL" pad="1"/>
</signal>
<signal name="LED_OUT">
<contactref element="OUT" pad="TP"/>
<contactref element="D19" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="30"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="31"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="10K2" pad="1"/>
<contactref element="SEQ_BUTTON" pad="4"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="IN" pad="TP"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
</signal>
<signal name="D11">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="D13">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$43">
<contactref element="Q1" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="4"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="4"/>
<contactref element="D3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="4"/>
<contactref element="D4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="D4" pad="4"/>
<contactref element="D5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="D5" pad="4"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D6" pad="4"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="D7" pad="4"/>
<contactref element="D8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="D8" pad="4"/>
<contactref element="D9" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="D9" pad="4"/>
<contactref element="D10" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="D10" pad="4"/>
<contactref element="D11" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="D11" pad="4"/>
<contactref element="D12" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D12" pad="4"/>
<contactref element="D13" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D13" pad="4"/>
<contactref element="D14" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="D14" pad="4"/>
<contactref element="D15" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="D15" pad="4"/>
<contactref element="D16" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="D17" pad="1"/>
<contactref element="D16" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="D17" pad="4"/>
<contactref element="D18" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="D18" pad="4"/>
<contactref element="D19" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="XOUT">
<contactref element="U1" pad="23"/>
</signal>
<signal name="YOUT">
<contactref element="U1" pad="24"/>
<contactref element="ACCEL" pad="5"/>
</signal>
<signal name="ZOUT">
<contactref element="U1" pad="25"/>
</signal>
<signal name="AUD">
<contactref element="U1" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
