// UTFT_Textrotation_Demo 
// Copyright (C)2015 Rinky-Dink Electronics, Henning Karlsen. All right reserved
// web: http://www.RinkyDinkElectronics.com/
//
// This program is a demo of the textrotation-functions.
//
// This demo was made for modules with a screen resolution 
// of 320x240 pixels.
//
// This program requires the UTFT library.
//

#include <UTFT.h>

// Declare which fonts we will be using
extern uint8_t BigFont[];
extern uint8_t SevenSegNumFont[];

// Set the pins to the correct ones for your development shield
// ------------------------------------------------------------
// My chipKit Uno32/uC32 shield                : <display model>,38,39,40,41
// My chipKit Max32 shield                     : <display model>,82,83,84,85
// AquaLEDSource All in One Super Screw Shield : <display model>,82,83,84,85
//
// Remember to change the model parameter to suit your display module!
UTFT myGLCD(ITDB32S,82,83,84,85);

void setup()
{
  myGLCD.InitLCD();
  myGLCD.clrScr();
  myGLCD.setFont(BigFont);
}

void loop()
{
    myGLCD.print("Text rotation", 0, 0);
    myGLCD.setColor(0, 0, 255);
    myGLCD.print("0 degrees", 0, 16, 0);
    myGLCD.print("90 degrees", 319, 0, 90);
    myGLCD.print("180 degrees", 319, 239, 180);
    myGLCD.print("270 degrees", 0, 239, 270);

    myGLCD.setFont(SevenSegNumFont);
    myGLCD.setColor(0, 255, 0);
    myGLCD.print("45", 90, 100, 45);
    myGLCD.print("90", 200, 50, 90);
    myGLCD.print("180", 300, 200, 180);

  while (true) {};
}

