<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="-42" y1="20" x2="-42" y2="10" width="0" layer="20"/>
<wire x1="-42" y1="10" x2="106" y2="10" width="0" layer="20"/>
<wire x1="106" y1="10" x2="106" y2="20" width="0" layer="20"/>
<wire x1="106" y1="20" x2="-42" y2="20" width="0" layer="20"/>
<wire x1="-42" y1="25" x2="106" y2="25" width="0" layer="20"/>
<wire x1="106" y1="25" x2="106" y2="35" width="0" layer="20"/>
<wire x1="106" y1="35" x2="-42" y2="35" width="0" layer="20"/>
<wire x1="-42" y1="35" x2="-42" y2="25" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTERY-AA-KIT">
<description>&lt;h3&gt;BATTERY-AA-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTERY-AA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08316"/>
</element>
<element name="BAT2" library="SparkFun-Electromechanical" package="BATTERY-AA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08316"/>
</element>
<element name="BAT3" library="SparkFun-Electromechanical" package="BATTERY-AA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08316"/>
</element>
<element name="BAT4" library="SparkFun-Electromechanical" package="BATTERY-AA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08316"/>
</element>
</elements>
<signals>
<signal name="+">
<contactref element="BAT1" pad="PWR@1"/>
<contactref element="BAT3" pad="PWR@1"/>
</signal>
<signal name="-">
<contactref element="BAT2" pad="GND@1"/>
<contactref element="BAT4" pad="GND@1"/>
</signal>
<signal name="N$1">
<contactref element="BAT1" pad="GND@1"/>
<contactref element="BAT2" pad="PWR@1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
<contactref element="BAT3" pad="GND@1"/>
<contactref element="BAT4" pad="PWR@1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
</signals>
</board>
</drawing>
</eagle>
