<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="13.286603125" y1="2.128678125" x2="10.276559375" y2="1.3022375" width="0" layer="20" curve="-109.760827"/>
<wire x1="10.276559375" y1="1.3022375" x2="8.93875" y2="0.150240625" width="0" layer="20" curve="-35.523558"/>
<wire x1="8.93875" y1="0.150240625" x2="6.4426" y2="1.7587125" width="0" layer="20" curve="-113.00732"/>
<wire x1="6.4426" y1="1.7587125" x2="6.4426" y2="2.28565625" width="0" layer="20"/>
<wire x1="6.4426" y1="2.28565625" x2="5.148496875" y2="3.138596875" width="0" layer="20" curve="-118.743857"/>
<wire x1="5.148496875" y1="3.138596875" x2="5.148496875" y2="3.4954" width="0" layer="20"/>
<wire x1="3.585209375" y1="7.934659375" x2="1.72076875" y2="10.36033125" width="0" layer="20" curve="-23.855579"/>
<wire x1="1.72076875" y1="10.36033125" x2="3.585209375" y2="26.46139375" width="0" layer="20" curve="-70.556918"/>
<wire x1="3.585209375" y1="26.46139375" x2="3.585209375" y2="28.295415625" width="0" layer="20"/>
<wire x1="3.585209375" y1="28.295415625" x2="26.381584375" y2="28.295415625" width="0" layer="20" curve="-180"/>
<wire x1="26.381584375" y1="28.295415625" x2="26.381584375" y2="26.46139375" width="0" layer="20"/>
<wire x1="26.381584375" y1="26.46139375" x2="28.246025" y2="10.36033125" width="0" layer="20" curve="-70.556918"/>
<wire x1="28.246025" y1="10.36033125" x2="26.381584375" y2="7.934659375" width="0" layer="20" curve="-23.855579"/>
<wire x1="26.381584375" y1="7.934659375" x2="26.381584375" y2="3.4954" width="0" layer="20"/>
<wire x1="26.381584375" y1="3.4954" x2="24.818296875" y2="3.4954" width="0" layer="20"/>
<wire x1="24.818296875" y1="3.4954" x2="24.818296875" y2="3.138596875" width="0" layer="20"/>
<wire x1="24.818296875" y1="3.138596875" x2="23.52419375" y2="2.28565625" width="0" layer="20" curve="-118.743857"/>
<wire x1="23.52419375" y1="2.28565625" x2="23.52419375" y2="1.7587125" width="0" layer="20"/>
<wire x1="23.52419375" y1="1.7587125" x2="21.02804375" y2="0.150240625" width="0" layer="20" curve="-113.00732"/>
<wire x1="21.02804375" y1="0.150240625" x2="19.69023125" y2="1.3022375" width="0" layer="20" curve="-35.523558"/>
<wire x1="19.69023125" y1="1.3022375" x2="16.6801875" y2="2.128678125" width="0" layer="20" curve="-109.760827"/>
<wire x1="16.6801875" y1="2.128678125" x2="13.286603125" y2="2.128678125" width="0" layer="20" curve="-10.997652"/>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>LONG
LEADS</text>
<text>TIE TACK</text>
<hole x="14.986" y="30.861" drill="1"/>
<wire x1="3.585209375" y1="3.4954" x2="3.585209375" y2="7.934659375" width="0" layer="20"/>
<wire x1="3.585209375" y1="3.4954" x2="5.148496875" y2="3.4954" width="0" layer="20"/>
<text>CR1220
BATTERY</text>
<text>+
SIDE UP</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SIMPLE_HOLE_SM">
<description>&lt;h3&gt;Simple Hole - Small&lt;/h3&gt;
Sew hole small diameter
&lt;p&gt;Specifications:
&lt;li&gt;Drill: 0.07in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEW_HOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
<description>&lt;h3&gt;12mm Coin Cell (CR1225) Battery Holder - SMD&lt;/h3&gt;
&lt;p&gt;Holds battery in place with friction. The metal housing connects to the positive side of the battery and the PCB pad underneath is connected to the negative side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3000.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TIETACK" library="SparkFun-Retired" package="SIMPLE_HOLE_SM" value="">
<attribute name="VALUE"/>
</element>
<element name="CR1220" library="SparkFun-Batteries" package="BATTCON_12MM" value="">
<attribute name="PROD_ID" value="BATT-08044"/>
<attribute name="SF_SKU" value="PRT-10592"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="CR1220" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="CR1220" pad="PWR@1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
