<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="145.291962962963" y2="0" width="0" layer="20"/>
<wire x1="145.291962962963" y1="0" x2="145.291962962963" y2="57.774416666666674" width="0" layer="20"/>
<wire x1="145.291962962963" y1="57.774416666666674" x2="0" y2="57.774416666666674" width="0" layer="20"/>
<wire x1="0" y1="57.774416666666674" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="Tinkercad">
<packages>
<package name="HA-06-SM065"></package>
<package name="CAP-THRU-2.54MM"></package>
<package name="LEDRD254W60D565H860B"><description>Radial LED (Round), 2.54 mm pitch, 5.65 mm body diameter, 8.60 mm body height
&lt;p&gt;Radial LED (Round) package with 2.54 mm pitch (lead spacing), 0.60 mm lead width, 0.50 mm lead thickness, 5.65 mm body diameter and 8.60 mm body height&lt;/p&gt;</description></package>
<package name="TO220BV"><description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description></package>
<package name="BATTERY-GENERIC"></package>
<package name="78F01T"></package>
<package name="MOTOR"></package>
<package name="RESAD1016W63L850D250B"><description>Axial Resistor, 10.16 mm pitch, 8.50 mm body length, 2.50 mm body diameter
 &lt;p&gt;Axial Resistor package with 10.16 mm pitch (lead spacing), 0.63 mm lead diameter, 8.50 mm body length and 2.50 mm body diameter&lt;/p&gt;</description></package>
<package name="PIEZO"><description>Radial Non-Polarized Inductor, 7.00 mm pitch, 17.00 mm body diameter, 11.00 mm body height
 &lt;p&gt;Radial Non-Polarized Inductor package with 7.00 mm pitch (lead spacing), 0.80 mm lead diameter, 17.00 mm body diameter and 11.00 mm body height&lt;/p&gt;</description></package>
</packages>
</library></libraries>
<attributes/>
<variantdefs/>
<elements>
<element name="SWON_OFF_SWITCH" library="Tinkercad" package="78F01T" value="DPST78F01T"/>
<element name="BAT1" library="Tinkercad" package="BATTERY-GENERIC" value="6V"/>
<element name="MSPINNER_MOTOR" library="Tinkercad" package="MOTOR" value="MOTOR_HDR"/>
<element name="TMOTOR_CONTROLLER_MOSFET" library="Tinkercad" package="TO220BV" value="NMOSFET">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE" value="NMOSFET"/>
</element>
<element name="R1M_RES" library="Tinkercad" package="RESAD1016W63L850D250B" value="1M"/>
<element name="RPOTMOTOR_SPEED_POT1" library="Tinkercad" package="HA-06-SM065" value="10k"/>
<element name="R2" library="Tinkercad" package="RESAD1016W63L850D250B" value="470"/>
<element name="DPOWER_LED" library="Tinkercad" package="LEDRD254W60D565H860B" value="RED">
<attribute name="CATEGORY" value="Opto-Electronic"/>
<attribute name="COLOR" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="LED"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE" value="LED_RED"/>
</element>
<element name="SWBUZZER_SWITCH" library="Tinkercad" package="78F01T" value="DPST78F01T"/>
<element name="PIEZO1" library="Tinkercad" package="PIEZO" value="PIEZO"/>
<element name="CBUZZER_CAPACITOR" library="Tinkercad" package="CAP-THRU-2.54MM" value="2000u"/>
</elements>
<signals>
<signal name="BAT1+">
<contactref element="BAT1" pad="+"/>
<contactref element="SWON_OFF_SWITCH" pad="2"/>
</signal>
<signal name="SWON_OFF_SWITCH_3">
<contactref element="PIEZO1" pad="1"/>
<contactref element="CBUZZER_CAPACITOR" pad="1"/>
<contactref element="DPOWER_LED" pad="1"/>
<contactref element="SWON_OFF_SWITCH" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="TMOTOR_CONTROLLER_MOSFET" pad="D"/>
</signal>
<signal name="BAT1-">
<contactref element="DPOWER_LED" pad="2"/>
<contactref element="BAT1" pad="-"/>
<contactref element="RPOTMOTOR_SPEED_POT1" pad="1"/>
<contactref element="MSPINNER_MOTOR" pad="-"/>
<contactref element="R1M_RES" pad="1"/>
<contactref element="SWBUZZER_SWITCH" pad="2"/>
</signal>
<signal name="MSPINNER_MOTOR_+">
<contactref element="MSPINNER_MOTOR" pad="+"/>
<contactref element="TMOTOR_CONTROLLER_MOSFET" pad="S"/>
</signal>
<signal name="TMOTOR_CONTROLLER_MOSFET_G">
<contactref element="RPOTMOTOR_SPEED_POT1" pad="2"/>
<contactref element="TMOTOR_CONTROLLER_MOSFET" pad="G"/>
<contactref element="R1M_RES" pad="2"/>
</signal>
<signal name="R2_2">
<contactref element="R2" pad="2"/>
<contactref element="RPOTMOTOR_SPEED_POT1" pad="3"/>
</signal>
<signal name="SWBUZZER_SWITCH_3">
<contactref element="CBUZZER_CAPACITOR" pad="2"/>
<contactref element="PIEZO1" pad="2"/>
<contactref element="SWBUZZER_SWITCH" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>