<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<circle x="2.54" y="2.54" radius="1.79605" width="0.4064" layer="20"/>
<wire x1="0" y1="0" x2="74.93" y2="0" width="0.4064" layer="20"/>
<wire x1="74.93" y1="0" x2="74.93" y2="82.55" width="0.4064" layer="20"/>
<wire x1="74.93" y1="82.55" x2="0" y2="82.55" width="0.4064" layer="20"/>
<wire x1="0" y1="82.55" x2="0" y2="0" width="0.4064" layer="20"/>
<circle x="72.39" y="2.54" radius="1.79605" width="0.4064" layer="20"/>
<circle x="72.39" y="80.01" radius="1.79605" width="0.4064" layer="20"/>
<circle x="2.54" y="80.01" radius="1.79605" width="0.4064" layer="20"/>
<hole x="30.48" y="39.37" drill="2"/>
<hole x="45.72" y="39.37" drill="2"/>
<hole x="2.54" y="80.01" drill="3.2"/>
<hole x="72.39" y="80.01" drill="3.2"/>
<hole x="72.39" y="2.54" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<text>Nano</text>
<text>Aoshido</text>
<text>Signal</text>
<text>12v</text>
<text>GND</text>
<circle x="91.44" y="80.01" radius="1.79605" width="0.4064" layer="20"/>
<hole x="91.44" y="80.01" drill="3.2"/>
<wire x1="93.98" y1="82.55" x2="93.98" y2="48.26" width="0.7" layer="20"/>
<wire x1="93.98" y1="48.26" x2="77.47" y2="48.26" width="0.7" layer="20"/>
<wire x1="77.47" y1="48.26" x2="77.47" y2="82.55" width="0.7" layer="20"/>
<wire x1="77.47" y1="82.55" x2="93.98" y2="82.55" width="0.7" layer="20"/>
<text>50Ω</text>
<text>DC_JACK</text>
<text>END_X</text>
<text>END_Y</text>
<text>FAN1</text>
<text>FAN2</text>
<text>LASER</text>
<text>LM317</text>
<text>NPN</text>
<text>POWER</text>
<text>X_AXIS</text>
<text>X_MOTOR</text>
<text>Y_AXIS</text>
<text>Y_MOTOR</text>
<circle x="101.6" y="2.54" radius="1.79605" width="0.4064" layer="20"/>
<wire x1="99.06" y1="0" x2="173.99" y2="0" width="0.4064" layer="20"/>
<wire x1="173.99" y1="0" x2="173.99" y2="82.55" width="0.4064" layer="20"/>
<wire x1="173.99" y1="82.55" x2="99.06" y2="82.55" width="0.4064" layer="20"/>
<wire x1="99.06" y1="82.55" x2="99.06" y2="0" width="0.4064" layer="20"/>
<circle x="171.45" y="2.54" radius="1.79605" width="0.4064" layer="20"/>
<circle x="171.45" y="80.01" radius="1.79605" width="0.4064" layer="20"/>
<circle x="101.6" y="80.01" radius="1.79605" width="0.4064" layer="20"/>
<hole x="129.54" y="39.37" drill="2"/>
<hole x="144.78" y="39.37" drill="2"/>
<hole x="101.6" y="80.01" drill="3.2"/>
<hole x="171.45" y="80.01" drill="3.2"/>
<hole x="171.45" y="2.54" drill="3.2"/>
<hole x="101.6" y="2.54" drill="3.2"/>
<hole x="101.6" y="2.54" drill="3.2"/>
<text>Nano</text>
<text>Aoshido</text>
<text>Signal</text>
<text>12v</text>
<text>GND</text>
<circle x="190.5" y="80.01" radius="1.79605" width="0.4064" layer="20"/>
<hole x="190.5" y="80.01" drill="3.2"/>
<wire x1="193.04" y1="82.55" x2="193.04" y2="48.26" width="0.7" layer="20"/>
<wire x1="193.04" y1="48.26" x2="176.53" y2="48.26" width="0.7" layer="20"/>
<wire x1="176.53" y1="48.26" x2="176.53" y2="82.55" width="0.7" layer="20"/>
<wire x1="176.53" y1="82.55" x2="193.04" y2="82.55" width="0.7" layer="20"/>
<text>50Ω</text>
<text>DC_JACK</text>
<text>END_X</text>
<text>END_Y</text>
<text>FAN1</text>
<text>FAN2</text>
<text>LASER</text>
<text>LM317</text>
<text>NPN</text>
<text>POWER</text>
<text>X_AXIS</text>
<text>X_MOTOR</text>
<text>Y_AXIS</text>
<text>Y_MOTOR</text>
<circle x="2.54" y="-99.06" radius="1.79605" width="0.4064" layer="20"/>
<wire x1="0" y1="-101.6" x2="74.93" y2="-101.6" width="0.4064" layer="20"/>
<wire x1="74.93" y1="-101.6" x2="74.93" y2="-19.05" width="0.4064" layer="20"/>
<wire x1="74.93" y1="-19.05" x2="0" y2="-19.05" width="0.4064" layer="20"/>
<wire x1="0" y1="-19.05" x2="0" y2="-101.6" width="0.4064" layer="20"/>
<circle x="72.39" y="-99.06" radius="1.79605" width="0.4064" layer="20"/>
<circle x="72.39" y="-21.59" radius="1.79605" width="0.4064" layer="20"/>
<circle x="2.54" y="-21.59" radius="1.79605" width="0.4064" layer="20"/>
<hole x="30.48" y="-62.23" drill="2"/>
<hole x="45.72" y="-62.23" drill="2"/>
<hole x="2.54" y="-21.59" drill="3.2"/>
<hole x="72.39" y="-21.59" drill="3.2"/>
<hole x="72.39" y="-99.06" drill="3.2"/>
<hole x="2.54" y="-99.06" drill="3.2"/>
<hole x="2.54" y="-99.06" drill="3.2"/>
<text>Nano</text>
<text>Aoshido</text>
<text>Signal</text>
<text>12v</text>
<text>GND</text>
<circle x="91.44" y="-21.59" radius="1.79605" width="0.4064" layer="20"/>
<hole x="91.44" y="-21.59" drill="3.2"/>
<wire x1="93.98" y1="-19.05" x2="93.98" y2="-53.34" width="0.7" layer="20"/>
<wire x1="93.98" y1="-53.34" x2="77.47" y2="-53.34" width="0.7" layer="20"/>
<wire x1="77.47" y1="-53.34" x2="77.47" y2="-19.05" width="0.7" layer="20"/>
<wire x1="77.47" y1="-19.05" x2="93.98" y2="-19.05" width="0.7" layer="20"/>
<text>50Ω</text>
<text>DC_JACK</text>
<text>END_X</text>
<text>END_Y</text>
<text>FAN1</text>
<text>FAN2</text>
<text>LASER</text>
<text>LM317</text>
<text>NPN</text>
<text>POWER</text>
<text>X_AXIS</text>
<text>X_MOTOR</text>
<text>Y_AXIS</text>
<text>Y_MOTOR</text>
<circle x="100.33" y="-99.06" radius="1.79605" width="0.4064" layer="20"/>
<wire x1="97.79" y1="-101.6" x2="172.72" y2="-101.6" width="0.4064" layer="20"/>
<wire x1="172.72" y1="-101.6" x2="172.72" y2="-19.05" width="0.4064" layer="20"/>
<wire x1="172.72" y1="-19.05" x2="97.79" y2="-19.05" width="0.4064" layer="20"/>
<wire x1="97.79" y1="-19.05" x2="97.79" y2="-101.6" width="0.4064" layer="20"/>
<circle x="170.18" y="-99.06" radius="1.79605" width="0.4064" layer="20"/>
<circle x="170.18" y="-21.59" radius="1.79605" width="0.4064" layer="20"/>
<circle x="100.33" y="-21.59" radius="1.79605" width="0.4064" layer="20"/>
<hole x="128.27" y="-62.23" drill="2"/>
<hole x="143.51" y="-62.23" drill="2"/>
<hole x="100.33" y="-21.59" drill="3.2"/>
<hole x="170.18" y="-21.59" drill="3.2"/>
<hole x="170.18" y="-99.06" drill="3.2"/>
<hole x="100.33" y="-99.06" drill="3.2"/>
<hole x="100.33" y="-99.06" drill="3.2"/>
<text>Nano</text>
<text>Aoshido</text>
<text>Signal</text>
<text>12v</text>
<text>GND</text>
<circle x="189.23" y="-21.59" radius="1.79605" width="0.4064" layer="20"/>
<hole x="189.23" y="-21.59" drill="3.2"/>
<wire x1="191.77" y1="-19.05" x2="191.77" y2="-53.34" width="0.7" layer="20"/>
<wire x1="191.77" y1="-53.34" x2="175.26" y2="-53.34" width="0.7" layer="20"/>
<wire x1="175.26" y1="-53.34" x2="175.26" y2="-19.05" width="0.7" layer="20"/>
<wire x1="175.26" y1="-19.05" x2="191.77" y2="-19.05" width="0.7" layer="20"/>
<text>50Ω</text>
<text>DC_JACK</text>
<text>END_X</text>
<text>END_Y</text>
<text>FAN1</text>
<text>FAN2</text>
<text>LASER</text>
<text>LM317</text>
<text>NPN</text>
<text>POWER</text>
<text>X_AXIS</text>
<text>X_MOTOR</text>
<text>Y_AXIS</text>
<text>Y_MOTOR</text>
</plain>
<libraries>
<library name="EasyDriver">
<packages>
<package name="EASYDRIVER_V44">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4001">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X15">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="0R/10">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-conrad">
<description>&lt;b&gt;Conrad Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="733980-62">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
DC20-09 (2.0 mm Center Pin)&lt;br&gt;
DC25-09 (2.5 mm Center Pin)&lt;br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/725000-749999/733980-da-01-en-Printbuchse_mit_Schaltkontakt_2mm.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="S63S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220AB">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
3-lead molded horzintal</description>
</package>
</packages>
</library>
<library name="discrete">
<description>Discrete devices (Antenna, Arrrester, Thermistor)</description>
<packages>
<package name="R-5">
<description>&lt;b&gt;Resistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Y_AXIS" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X_AXIS" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="1N4001" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="1N4001"/>
<element name="FAN1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_X" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_Y" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$2" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="pinhead" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="E$10" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$11" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$12" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="X_MOTOR" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y_MOTOR" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$15" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$16" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="DC_JACK" library="con-conrad" package="733980-62" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$14" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$1" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="SparkFun-Resistors" package="AXIAL-0.6" value="5Ω">
<attribute name="VALUE"/>
</element>
<element name="NPN" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$9" library="eagle-ltspice" package="0204/7" value="220Ω">
<attribute name="VALUE"/>
</element>
<element name="LASER" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="50Ω" library="pot" package="S63S" value=""/>
<element name="E$7" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="LM317" library="diode" package="TO220AB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$8" library="discrete" package="R-5" value="">
<attribute name="VALUE"/>
</element>
<element name="Y_AXIS1" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X_AXIS1" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="1N1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="1N4001"/>
<element name="FAN3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN4" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_X1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_Y1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$13" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$17" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$18" library="pinhead" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="E$19" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$20" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$21" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="X_MOTOR1" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y_MOTOR1" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$22" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$23" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="DC_JACK1" library="con-conrad" package="733980-62" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$24" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$25" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$26" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$27" library="SparkFun-Resistors" package="AXIAL-0.6" value="5Ω">
<attribute name="VALUE"/>
</element>
<element name="NPN1" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$28" library="eagle-ltspice" package="0204/7" value="220Ω">
<attribute name="VALUE"/>
</element>
<element name="LASER1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="50Ω1" library="pot" package="S63S" value=""/>
<element name="E$29" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="LM1" library="diode" package="TO220AB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$30" library="discrete" package="R-5" value="">
<attribute name="VALUE"/>
</element>
<element name="Y_AXIS2" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X_AXIS2" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="1N2" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="1N4001"/>
<element name="FAN5" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN6" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_X2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_Y2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$31" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$32" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$33" library="pinhead" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="E$34" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$35" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$36" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="X_MOTOR2" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y_MOTOR2" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$37" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$38" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="DC_JACK2" library="con-conrad" package="733980-62" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$39" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$40" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$41" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$42" library="SparkFun-Resistors" package="AXIAL-0.6" value="5Ω">
<attribute name="VALUE"/>
</element>
<element name="NPN2" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$43" library="eagle-ltspice" package="0204/7" value="220Ω">
<attribute name="VALUE"/>
</element>
<element name="LASER2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="50Ω2" library="pot" package="S63S" value=""/>
<element name="E$44" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="LM2" library="diode" package="TO220AB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$45" library="discrete" package="R-5" value="">
<attribute name="VALUE"/>
</element>
<element name="Y_AXIS3" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X_AXIS3" library="EasyDriver" package="EASYDRIVER_V44" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="1N3" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="1N4001"/>
<element name="FAN7" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN8" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_X3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="END_Y3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$46" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$47" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$48" library="pinhead" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="E$49" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$50" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$51" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="X_MOTOR3" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y_MOTOR3" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$52" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$53" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="DC_JACK3" library="con-conrad" package="733980-62" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$54" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="E$55" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$56" library="jumper" package="0R/10" value="">
<attribute name="VALUE"/>
</element>
<element name="E$57" library="SparkFun-Resistors" package="AXIAL-0.6" value="5Ω">
<attribute name="VALUE"/>
</element>
<element name="NPN3" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$58" library="eagle-ltspice" package="0204/7" value="220Ω">
<attribute name="VALUE"/>
</element>
<element name="LASER3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="50Ω3" library="pot" package="S63S" value=""/>
<element name="E$59" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="LM3" library="diode" package="TO220AB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$60" library="discrete" package="R-5" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="Y_AXIS" pad="STEP"/>
<contactref element="E$5" pad="10"/>
</signal>
<signal name="S$2">
<contactref element="X_AXIS" pad="STEP"/>
<contactref element="E$5" pad="11"/>
</signal>
<signal name="S$4">
<contactref element="Y_AXIS" pad="DIR"/>
<contactref element="E$5" pad="7"/>
</signal>
<signal name="S$5">
<contactref element="E$1" pad="2"/>
<contactref element="E$5" pad="8"/>
</signal>
<signal name="S$3">
<contactref element="X_AXIS" pad="DIR"/>
<contactref element="E$1" pad="1"/>
</signal>
<signal name="S$25">
<contactref element="Y_AXIS" pad="GND2"/>
<contactref element="Y_AXIS" pad="GND1"/>
<contactref element="E$12" pad="2"/>
</signal>
<signal name="S$16">
<contactref element="E$4" pad="1"/>
<contactref element="E$12" pad="1"/>
</signal>
<signal name="GND">
<contactref element="E$3" pad="2"/>
<contactref element="Y_AXIS" pad="GND3"/>
<contactref element="E$5" pad="12"/>
<contactref element="FAN1" pad="1"/>
<contactref element="FAN2" pad="1"/>
<contactref element="END_Y" pad="2"/>
<contactref element="X_AXIS" pad="GND3"/>
<contactref element="END_X" pad="2"/>
<contactref element="X_AXIS" pad="GND2"/>
<contactref element="X_AXIS" pad="GND1"/>
<contactref element="DC_JACK" pad="3"/>
<contactref element="E$14" pad="3"/>
<contactref element="DC_JACK" pad="2"/>
<contactref element="E$4" pad="2"/>
</signal>
<signal name="S$20">
<contactref element="Y_AXIS" pad="MS2"/>
<contactref element="Y_AXIS" pad="MS1"/>
<contactref element="Y_AXIS" pad="P$11"/>
</signal>
<signal name="5V">
<contactref element="X_AXIS" pad="P$11"/>
<contactref element="X_AXIS" pad="MS1"/>
<contactref element="X_AXIS" pad="MS2"/>
</signal>
<signal name="S$27">
<contactref element="Y_AXIS" pad="M+"/>
<contactref element="E$16" pad="1"/>
</signal>
<signal name="12V">
<contactref element="FAN1" pad="2"/>
<contactref element="FAN2" pad="2"/>
<contactref element="X_AXIS" pad="M+"/>
<contactref element="POWER" pad="1"/>
<contactref element="E$15" pad="2"/>
<contactref element="E$14" pad="2"/>
</signal>
<signal name="S$6">
<contactref element="E$5" pad="2"/>
<contactref element="E$14" pad="1"/>
</signal>
<signal name="S$17">
<contactref element="E$5" pad="3"/>
<contactref element="E$10" pad="2"/>
</signal>
<signal name="S$22">
<contactref element="POWER" pad="2"/>
<contactref element="1N4001" pad="C"/>
</signal>
<signal name="S$15">
<contactref element="E$5" pad="4"/>
<contactref element="E$11" pad="2"/>
</signal>
<signal name="S$23">
<contactref element="END_X" pad="1"/>
<contactref element="E$10" pad="1"/>
</signal>
<signal name="S$24">
<contactref element="E$11" pad="1"/>
<contactref element="END_Y" pad="1"/>
</signal>
<signal name="S$7">
<contactref element="Y_MOTOR" pad="4"/>
<contactref element="Y_AXIS" pad="B1"/>
</signal>
<signal name="S$8">
<contactref element="Y_MOTOR" pad="3"/>
<contactref element="Y_AXIS" pad="B2"/>
</signal>
<signal name="S$9">
<contactref element="Y_MOTOR" pad="2"/>
<contactref element="Y_AXIS" pad="A2"/>
</signal>
<signal name="S$10">
<contactref element="Y_MOTOR" pad="1"/>
<contactref element="Y_AXIS" pad="A1"/>
</signal>
<signal name="S$11">
<contactref element="X_MOTOR" pad="4"/>
<contactref element="X_AXIS" pad="B1"/>
</signal>
<signal name="S$12">
<contactref element="X_MOTOR" pad="3"/>
<contactref element="X_AXIS" pad="B2"/>
</signal>
<signal name="S$13">
<contactref element="X_MOTOR" pad="2"/>
<contactref element="X_AXIS" pad="A2"/>
</signal>
<signal name="S$14">
<contactref element="X_MOTOR" pad="1"/>
<contactref element="X_AXIS" pad="A1"/>
</signal>
<signal name="S$26">
<contactref element="E$15" pad="1"/>
<contactref element="E$16" pad="2"/>
</signal>
<signal name="S$19">
<contactref element="1N4001" pad="A"/>
<contactref element="DC_JACK" pad="1"/>
</signal>
<signal name="S$18">
</signal>
<signal name="GND1">
<contactref element="NPN" pad="1"/>
<contactref element="E$7" pad="2"/>
</signal>
<signal name="12V1">
<contactref element="E$7" pad="3"/>
<contactref element="LM317" pad="A1"/>
</signal>
<signal name="S$21">
<contactref element="E$6" pad="P$2"/>
<contactref element="LM317" pad="A2"/>
</signal>
<signal name="S$28">
<contactref element="NPN" pad="2"/>
<contactref element="E$9" pad="2"/>
</signal>
<signal name="S$29">
<contactref element="LASER" pad="1"/>
<contactref element="NPN" pad="3"/>
</signal>
<signal name="S$30">
<contactref element="E$6" pad="P$1"/>
<contactref element="50Ω" pad="A"/>
<contactref element="50Ω" pad="S"/>
</signal>
<signal name="S$31">
<contactref element="50Ω" pad="E"/>
<contactref element="LM317" pad="C"/>
<contactref element="LASER" pad="2"/>
</signal>
<signal name="S$32">
<contactref element="E$8" pad="1"/>
<contactref element="E$7" pad="1"/>
</signal>
<signal name="S$33">
<contactref element="E$9" pad="1"/>
<contactref element="E$8" pad="2"/>
</signal>
<signal name="S$34">
</signal>
<signal name="S$35">
<contactref element="Y_AXIS1" pad="STEP"/>
<contactref element="E$18" pad="10"/>
</signal>
<signal name="S$36">
<contactref element="X_AXIS1" pad="STEP"/>
<contactref element="E$18" pad="11"/>
</signal>
<signal name="S$37">
<contactref element="Y_AXIS1" pad="DIR"/>
<contactref element="E$18" pad="7"/>
</signal>
<signal name="S$38">
<contactref element="E$25" pad="2"/>
<contactref element="E$18" pad="8"/>
</signal>
<signal name="S$39">
<contactref element="X_AXIS1" pad="DIR"/>
<contactref element="E$25" pad="1"/>
</signal>
<signal name="S$40">
<contactref element="Y_AXIS1" pad="GND2"/>
<contactref element="Y_AXIS1" pad="GND1"/>
<contactref element="E$21" pad="2"/>
</signal>
<signal name="S$41">
<contactref element="E$26" pad="1"/>
<contactref element="E$21" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="E$17" pad="2"/>
<contactref element="Y_AXIS1" pad="GND3"/>
<contactref element="E$18" pad="12"/>
<contactref element="FAN3" pad="1"/>
<contactref element="FAN4" pad="1"/>
<contactref element="END_Y1" pad="2"/>
<contactref element="X_AXIS1" pad="GND3"/>
<contactref element="END_X1" pad="2"/>
<contactref element="X_AXIS1" pad="GND2"/>
<contactref element="X_AXIS1" pad="GND1"/>
<contactref element="DC_JACK1" pad="3"/>
<contactref element="E$24" pad="3"/>
<contactref element="DC_JACK1" pad="2"/>
<contactref element="E$26" pad="2"/>
</signal>
<signal name="S$42">
<contactref element="Y_AXIS1" pad="MS2"/>
<contactref element="Y_AXIS1" pad="MS1"/>
<contactref element="Y_AXIS1" pad="P$11"/>
</signal>
<signal name="5V1">
<contactref element="X_AXIS1" pad="P$11"/>
<contactref element="X_AXIS1" pad="MS1"/>
<contactref element="X_AXIS1" pad="MS2"/>
</signal>
<signal name="S$43">
<contactref element="Y_AXIS1" pad="M+"/>
<contactref element="E$23" pad="1"/>
</signal>
<signal name="12V2">
<contactref element="FAN3" pad="2"/>
<contactref element="FAN4" pad="2"/>
<contactref element="X_AXIS1" pad="M+"/>
<contactref element="POWER1" pad="1"/>
<contactref element="E$22" pad="2"/>
<contactref element="E$24" pad="2"/>
</signal>
<signal name="S$44">
<contactref element="E$18" pad="2"/>
<contactref element="E$24" pad="1"/>
</signal>
<signal name="S$45">
<contactref element="E$18" pad="3"/>
<contactref element="E$19" pad="2"/>
</signal>
<signal name="S$46">
<contactref element="POWER1" pad="2"/>
<contactref element="1N1" pad="C"/>
</signal>
<signal name="S$47">
<contactref element="E$18" pad="4"/>
<contactref element="E$20" pad="2"/>
</signal>
<signal name="S$48">
<contactref element="END_X1" pad="1"/>
<contactref element="E$19" pad="1"/>
</signal>
<signal name="S$49">
<contactref element="E$20" pad="1"/>
<contactref element="END_Y1" pad="1"/>
</signal>
<signal name="S$50">
<contactref element="Y_MOTOR1" pad="4"/>
<contactref element="Y_AXIS1" pad="B1"/>
</signal>
<signal name="S$51">
<contactref element="Y_MOTOR1" pad="3"/>
<contactref element="Y_AXIS1" pad="B2"/>
</signal>
<signal name="S$52">
<contactref element="Y_MOTOR1" pad="2"/>
<contactref element="Y_AXIS1" pad="A2"/>
</signal>
<signal name="S$53">
<contactref element="Y_MOTOR1" pad="1"/>
<contactref element="Y_AXIS1" pad="A1"/>
</signal>
<signal name="S$54">
<contactref element="X_MOTOR1" pad="4"/>
<contactref element="X_AXIS1" pad="B1"/>
</signal>
<signal name="S$55">
<contactref element="X_MOTOR1" pad="3"/>
<contactref element="X_AXIS1" pad="B2"/>
</signal>
<signal name="S$56">
<contactref element="X_MOTOR1" pad="2"/>
<contactref element="X_AXIS1" pad="A2"/>
</signal>
<signal name="S$57">
<contactref element="X_MOTOR1" pad="1"/>
<contactref element="X_AXIS1" pad="A1"/>
</signal>
<signal name="S$58">
<contactref element="E$22" pad="1"/>
<contactref element="E$23" pad="2"/>
</signal>
<signal name="S$59">
<contactref element="1N1" pad="A"/>
<contactref element="DC_JACK1" pad="1"/>
</signal>
<signal name="S$60">
</signal>
<signal name="GND3">
<contactref element="NPN1" pad="1"/>
<contactref element="E$29" pad="2"/>
</signal>
<signal name="12V3">
<contactref element="E$29" pad="3"/>
<contactref element="LM1" pad="A1"/>
</signal>
<signal name="S$61">
<contactref element="E$27" pad="P$2"/>
<contactref element="LM1" pad="A2"/>
</signal>
<signal name="S$62">
<contactref element="NPN1" pad="2"/>
<contactref element="E$28" pad="2"/>
</signal>
<signal name="S$63">
<contactref element="LASER1" pad="1"/>
<contactref element="NPN1" pad="3"/>
</signal>
<signal name="S$64">
<contactref element="E$27" pad="P$1"/>
<contactref element="50Ω1" pad="A"/>
<contactref element="50Ω1" pad="S"/>
</signal>
<signal name="S$65">
<contactref element="50Ω1" pad="E"/>
<contactref element="LM1" pad="C"/>
<contactref element="LASER1" pad="2"/>
</signal>
<signal name="S$66">
<contactref element="E$30" pad="1"/>
<contactref element="E$29" pad="1"/>
</signal>
<signal name="S$67">
<contactref element="E$28" pad="1"/>
<contactref element="E$30" pad="2"/>
</signal>
<signal name="S$68">
</signal>
<signal name="S$69">
<contactref element="Y_AXIS2" pad="STEP"/>
<contactref element="E$33" pad="10"/>
</signal>
<signal name="S$70">
<contactref element="X_AXIS2" pad="STEP"/>
<contactref element="E$33" pad="11"/>
</signal>
<signal name="S$71">
<contactref element="Y_AXIS2" pad="DIR"/>
<contactref element="E$33" pad="7"/>
</signal>
<signal name="S$72">
<contactref element="E$40" pad="2"/>
<contactref element="E$33" pad="8"/>
</signal>
<signal name="S$73">
<contactref element="X_AXIS2" pad="DIR"/>
<contactref element="E$40" pad="1"/>
</signal>
<signal name="S$74">
<contactref element="Y_AXIS2" pad="GND2"/>
<contactref element="Y_AXIS2" pad="GND1"/>
<contactref element="E$36" pad="2"/>
</signal>
<signal name="S$75">
<contactref element="E$41" pad="1"/>
<contactref element="E$36" pad="1"/>
</signal>
<signal name="GND4">
<contactref element="E$32" pad="2"/>
<contactref element="Y_AXIS2" pad="GND3"/>
<contactref element="E$33" pad="12"/>
<contactref element="FAN5" pad="1"/>
<contactref element="FAN6" pad="1"/>
<contactref element="END_Y2" pad="2"/>
<contactref element="X_AXIS2" pad="GND3"/>
<contactref element="END_X2" pad="2"/>
<contactref element="X_AXIS2" pad="GND2"/>
<contactref element="X_AXIS2" pad="GND1"/>
<contactref element="DC_JACK2" pad="3"/>
<contactref element="E$39" pad="3"/>
<contactref element="DC_JACK2" pad="2"/>
<contactref element="E$41" pad="2"/>
</signal>
<signal name="S$76">
<contactref element="Y_AXIS2" pad="MS2"/>
<contactref element="Y_AXIS2" pad="MS1"/>
<contactref element="Y_AXIS2" pad="P$11"/>
</signal>
<signal name="5V2">
<contactref element="X_AXIS2" pad="P$11"/>
<contactref element="X_AXIS2" pad="MS1"/>
<contactref element="X_AXIS2" pad="MS2"/>
</signal>
<signal name="S$77">
<contactref element="Y_AXIS2" pad="M+"/>
<contactref element="E$38" pad="1"/>
</signal>
<signal name="12V4">
<contactref element="FAN5" pad="2"/>
<contactref element="FAN6" pad="2"/>
<contactref element="X_AXIS2" pad="M+"/>
<contactref element="POWER2" pad="1"/>
<contactref element="E$37" pad="2"/>
<contactref element="E$39" pad="2"/>
</signal>
<signal name="S$78">
<contactref element="E$33" pad="2"/>
<contactref element="E$39" pad="1"/>
</signal>
<signal name="S$79">
<contactref element="E$33" pad="3"/>
<contactref element="E$34" pad="2"/>
</signal>
<signal name="S$80">
<contactref element="POWER2" pad="2"/>
<contactref element="1N2" pad="C"/>
</signal>
<signal name="S$81">
<contactref element="E$33" pad="4"/>
<contactref element="E$35" pad="2"/>
</signal>
<signal name="S$82">
<contactref element="END_X2" pad="1"/>
<contactref element="E$34" pad="1"/>
</signal>
<signal name="S$83">
<contactref element="E$35" pad="1"/>
<contactref element="END_Y2" pad="1"/>
</signal>
<signal name="S$84">
<contactref element="Y_MOTOR2" pad="4"/>
<contactref element="Y_AXIS2" pad="B1"/>
</signal>
<signal name="S$85">
<contactref element="Y_MOTOR2" pad="3"/>
<contactref element="Y_AXIS2" pad="B2"/>
</signal>
<signal name="S$86">
<contactref element="Y_MOTOR2" pad="2"/>
<contactref element="Y_AXIS2" pad="A2"/>
</signal>
<signal name="S$87">
<contactref element="Y_MOTOR2" pad="1"/>
<contactref element="Y_AXIS2" pad="A1"/>
</signal>
<signal name="S$88">
<contactref element="X_MOTOR2" pad="4"/>
<contactref element="X_AXIS2" pad="B1"/>
</signal>
<signal name="S$89">
<contactref element="X_MOTOR2" pad="3"/>
<contactref element="X_AXIS2" pad="B2"/>
</signal>
<signal name="S$90">
<contactref element="X_MOTOR2" pad="2"/>
<contactref element="X_AXIS2" pad="A2"/>
</signal>
<signal name="S$91">
<contactref element="X_MOTOR2" pad="1"/>
<contactref element="X_AXIS2" pad="A1"/>
</signal>
<signal name="S$92">
<contactref element="E$37" pad="1"/>
<contactref element="E$38" pad="2"/>
</signal>
<signal name="S$93">
<contactref element="1N2" pad="A"/>
<contactref element="DC_JACK2" pad="1"/>
</signal>
<signal name="S$94">
</signal>
<signal name="GND5">
<contactref element="NPN2" pad="1"/>
<contactref element="E$44" pad="2"/>
</signal>
<signal name="12V5">
<contactref element="E$44" pad="3"/>
<contactref element="LM2" pad="A1"/>
</signal>
<signal name="S$95">
<contactref element="E$42" pad="P$2"/>
<contactref element="LM2" pad="A2"/>
</signal>
<signal name="S$96">
<contactref element="NPN2" pad="2"/>
<contactref element="E$43" pad="2"/>
</signal>
<signal name="S$97">
<contactref element="LASER2" pad="1"/>
<contactref element="NPN2" pad="3"/>
</signal>
<signal name="S$98">
<contactref element="E$42" pad="P$1"/>
<contactref element="50Ω2" pad="A"/>
<contactref element="50Ω2" pad="S"/>
</signal>
<signal name="S$99">
<contactref element="50Ω2" pad="E"/>
<contactref element="LM2" pad="C"/>
<contactref element="LASER2" pad="2"/>
</signal>
<signal name="S$100">
<contactref element="E$45" pad="1"/>
<contactref element="E$44" pad="1"/>
</signal>
<signal name="S$101">
<contactref element="E$43" pad="1"/>
<contactref element="E$45" pad="2"/>
</signal>
<signal name="S$102">
</signal>
<signal name="S$103">
<contactref element="Y_AXIS3" pad="STEP"/>
<contactref element="E$48" pad="10"/>
</signal>
<signal name="S$104">
<contactref element="X_AXIS3" pad="STEP"/>
<contactref element="E$48" pad="11"/>
</signal>
<signal name="S$105">
<contactref element="Y_AXIS3" pad="DIR"/>
<contactref element="E$48" pad="7"/>
</signal>
<signal name="S$106">
<contactref element="E$55" pad="2"/>
<contactref element="E$48" pad="8"/>
</signal>
<signal name="S$107">
<contactref element="X_AXIS3" pad="DIR"/>
<contactref element="E$55" pad="1"/>
</signal>
<signal name="S$108">
<contactref element="Y_AXIS3" pad="GND2"/>
<contactref element="Y_AXIS3" pad="GND1"/>
<contactref element="E$51" pad="2"/>
</signal>
<signal name="S$109">
<contactref element="E$56" pad="1"/>
<contactref element="E$51" pad="1"/>
</signal>
<signal name="GND6">
<contactref element="E$47" pad="2"/>
<contactref element="Y_AXIS3" pad="GND3"/>
<contactref element="E$48" pad="12"/>
<contactref element="FAN7" pad="1"/>
<contactref element="FAN8" pad="1"/>
<contactref element="END_Y3" pad="2"/>
<contactref element="X_AXIS3" pad="GND3"/>
<contactref element="END_X3" pad="2"/>
<contactref element="X_AXIS3" pad="GND2"/>
<contactref element="X_AXIS3" pad="GND1"/>
<contactref element="DC_JACK3" pad="3"/>
<contactref element="E$54" pad="3"/>
<contactref element="DC_JACK3" pad="2"/>
<contactref element="E$56" pad="2"/>
</signal>
<signal name="S$110">
<contactref element="Y_AXIS3" pad="MS2"/>
<contactref element="Y_AXIS3" pad="MS1"/>
<contactref element="Y_AXIS3" pad="P$11"/>
</signal>
<signal name="5V3">
<contactref element="X_AXIS3" pad="P$11"/>
<contactref element="X_AXIS3" pad="MS1"/>
<contactref element="X_AXIS3" pad="MS2"/>
</signal>
<signal name="S$111">
<contactref element="Y_AXIS3" pad="M+"/>
<contactref element="E$53" pad="1"/>
</signal>
<signal name="12V6">
<contactref element="FAN7" pad="2"/>
<contactref element="FAN8" pad="2"/>
<contactref element="X_AXIS3" pad="M+"/>
<contactref element="POWER3" pad="1"/>
<contactref element="E$52" pad="2"/>
<contactref element="E$54" pad="2"/>
</signal>
<signal name="S$112">
<contactref element="E$48" pad="2"/>
<contactref element="E$54" pad="1"/>
</signal>
<signal name="S$113">
<contactref element="E$48" pad="3"/>
<contactref element="E$49" pad="2"/>
</signal>
<signal name="S$114">
<contactref element="POWER3" pad="2"/>
<contactref element="1N3" pad="C"/>
</signal>
<signal name="S$115">
<contactref element="E$48" pad="4"/>
<contactref element="E$50" pad="2"/>
</signal>
<signal name="S$116">
<contactref element="END_X3" pad="1"/>
<contactref element="E$49" pad="1"/>
</signal>
<signal name="S$117">
<contactref element="E$50" pad="1"/>
<contactref element="END_Y3" pad="1"/>
</signal>
<signal name="S$118">
<contactref element="Y_MOTOR3" pad="4"/>
<contactref element="Y_AXIS3" pad="B1"/>
</signal>
<signal name="S$119">
<contactref element="Y_MOTOR3" pad="3"/>
<contactref element="Y_AXIS3" pad="B2"/>
</signal>
<signal name="S$120">
<contactref element="Y_MOTOR3" pad="2"/>
<contactref element="Y_AXIS3" pad="A2"/>
</signal>
<signal name="S$121">
<contactref element="Y_MOTOR3" pad="1"/>
<contactref element="Y_AXIS3" pad="A1"/>
</signal>
<signal name="S$122">
<contactref element="X_MOTOR3" pad="4"/>
<contactref element="X_AXIS3" pad="B1"/>
</signal>
<signal name="S$123">
<contactref element="X_MOTOR3" pad="3"/>
<contactref element="X_AXIS3" pad="B2"/>
</signal>
<signal name="S$124">
<contactref element="X_MOTOR3" pad="2"/>
<contactref element="X_AXIS3" pad="A2"/>
</signal>
<signal name="S$125">
<contactref element="X_MOTOR3" pad="1"/>
<contactref element="X_AXIS3" pad="A1"/>
</signal>
<signal name="S$126">
<contactref element="E$52" pad="1"/>
<contactref element="E$53" pad="2"/>
</signal>
<signal name="S$127">
<contactref element="1N3" pad="A"/>
<contactref element="DC_JACK3" pad="1"/>
</signal>
<signal name="S$128">
</signal>
<signal name="GND7">
<contactref element="NPN3" pad="1"/>
<contactref element="E$59" pad="2"/>
</signal>
<signal name="12V7">
<contactref element="E$59" pad="3"/>
<contactref element="LM3" pad="A1"/>
</signal>
<signal name="S$129">
<contactref element="E$57" pad="P$2"/>
<contactref element="LM3" pad="A2"/>
</signal>
<signal name="S$130">
<contactref element="NPN3" pad="2"/>
<contactref element="E$58" pad="2"/>
</signal>
<signal name="S$131">
<contactref element="LASER3" pad="1"/>
<contactref element="NPN3" pad="3"/>
</signal>
<signal name="S$132">
<contactref element="E$57" pad="P$1"/>
<contactref element="50Ω3" pad="A"/>
<contactref element="50Ω3" pad="S"/>
</signal>
<signal name="S$133">
<contactref element="50Ω3" pad="E"/>
<contactref element="LM3" pad="C"/>
<contactref element="LASER3" pad="2"/>
</signal>
<signal name="S$134">
<contactref element="E$60" pad="1"/>
<contactref element="E$59" pad="1"/>
</signal>
<signal name="S$135">
<contactref element="E$58" pad="1"/>
<contactref element="E$60" pad="2"/>
</signal>
<signal name="S$136">
</signal>
</signals>
</board>
</drawing>
</eagle>
