<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<!--Created by TARGET 3001! Version: 32.4.0.23-->
<!--DateTime: 2024/05/12 08:50:28-->
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="39.445" y1="0" x2="39.445" y2="34.925" width="0.3" layer="20"/>
<wire x1="4.445" y1="0" x2="39.445" y2="0" width="0.3" layer="20"/>
<wire x1="39.445" y1="34.925" x2="4.445" y2="34.925" width="0.3" layer="20"/>
<wire x1="4.445" y1="34.925" x2="4.445" y2="0" width="0.3" layer="20"/>
<text>Current Project from TARGET NC edition: Commercial use is criminal!</text>
</plain>
<libraries>
<library name="TARGET3001!_V32.4.0.23">
<packages>
<package name="SO8_SOT96-1">
</package>
<package name="1210">
</package>
<package name="6X11R7,62">
</package>
<package name="0204_MET">
</package>
<package name="1206">
</package>
<package name="WEMOS_D1">
</package>
<package name="LED_3MM_WEIß">
</package>
<package name="MIC_CMC-9745-44P_CUD">
</package>
<package name="HLK-PM01(#1)">
</package>
<package name="VISHAY_64W">
</package>
</packages>
</library>
</libraries>
<attributes/>
<variantdefs>
<variantdef name="&lt;unnamed&gt;"/>
</variantdefs>
<elements>
<element name="U1" library="TARGET3001!_V32.4.0.23" package="SO8_SOT96-1" value="NE567D"/>
<element name="C3" library="TARGET3001!_V32.4.0.23" package="1210" value="10�F"/>
<element name="C6" library="TARGET3001!_V32.4.0.23" package="1210" value="22�F"/>
<element name="C5" library="TARGET3001!_V32.4.0.23" package="1210" value="100nF"/>
<element name="C1" library="TARGET3001!_V32.4.0.23" package="6X11R7,62" value="100nF"/>
<element name="C2" library="TARGET3001!_V32.4.0.23" package="1210" value="220nF"/>
<element name="R1" library="TARGET3001!_V32.4.0.23" package="0204_MET" value="2,7K"/>
<element name="R2" library="TARGET3001!_V32.4.0.23" package="1206" value="10K"/>
<element name="C4" library="TARGET3001!_V32.4.0.23" package="1206" value="2.2�F"/>
<element name="U2" library="TARGET3001!_V32.4.0.23" package="WEMOS_D1" value="Wemos_D1_mini"/>
<element name="R3" library="TARGET3001!_V32.4.0.23" package="1206" value="10K"/>
<element name="U3" library="TARGET3001!_V32.4.0.23" package="SO8_SOT96-1" value="OPA340UA"/>
<element name="C7" library="TARGET3001!_V32.4.0.23" package="1206" value="2.2�F"/>
<element name="C8" library="TARGET3001!_V32.4.0.23" package="1206" value="2.2�F"/>
<element name="R4" library="TARGET3001!_V32.4.0.23" package="1206" value="68k"/>
<element name="R5" library="TARGET3001!_V32.4.0.23" package="1206" value="10K"/>
<element name="R6" library="TARGET3001!_V32.4.0.23" package="1206" value="10K"/>
<element name="C9" library="TARGET3001!_V32.4.0.23" package="1210" value="22pF"/>
<element name="R7" library="TARGET3001!_V32.4.0.23" package="1206" value="6k8"/>
<element name="D1" library="TARGET3001!_V32.4.0.23" package="LED_3MM_WEIß" value="LED-3-WH-DIF">
<attribute name="NAME"/>
</element>
<element name="R8" library="TARGET3001!_V32.4.0.23" package="1206" value="220"/>
<element name="MIC1" library="TARGET3001!_V32.4.0.23" package="MIC_CMC-9745-44P_CUD" value="CMC-9745-44P"/>
<element name="U4" library="TARGET3001!_V32.4.0.23" package="HLK-PM01(#1)" value="HLK-PM01"/>
<element name="R9" library="TARGET3001!_V32.4.0.23" package="VISHAY_64W" value="1K"/>
</elements>
<signals>
<signal name="IN"/>
<signal name="SIG$2"/>
<signal name="SIG$3"/>
<signal name="SIG$9"/>
<signal name="C1"/>
<signal name="SIG$12"/>
<signal name="SIG$13"/>
<signal name="+"/>
<signal name="SIG$15"/>
<signal name="OUT">
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="SIG$17"/>
<signal name="+5V"/>
<signal name="SIG$19"/>
<signal name="SIG$20"/>
<signal name="SIG$22"/>
<signal name="SIG$23"/>
<signal name="SIG$24"/>
<signal name="GND">
<contactref element="U1" pad="7"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="15"/>
<contactref element="U3" pad="4"/>
<contactref element="C8" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="MIC1" pad="2"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="SIG$27"/>
<signal name="5"/>
<signal name="SIG$36"/>
<signal name="SIG$40"/>
<signal name="4"/>
<signal name="SIG$44"/>
<signal name="SIG$46"/>
<signal name="R1"/>
<signal name="SIG$49"/>
<signal name="SIG$50"/>
<signal name="SIG$51"/>
<signal name="SIG$52"/>
<signal name="IN_2"/>
<signal name="SIG$54"/>
<signal name="SIG$55"/>
<signal name="OUT_2"/>
<signal name="SIG$57"/>
<signal name="SIG$58"/>
<signal name="2"/>
<signal name="SIG$60"/>
<signal name="SIG$61"/>
<signal name="SIG$62"/>
<signal name="SIG$64"/>
<signal name="SIG$65"/>
<signal name="PIN1">
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="MIC1" pad="1"/>
</signal>
<signal name="SIG$70"/>
<signal name="SIG$71"/>
<signal name="SIG$72"/>
<signal name="SIG$73"/>
<signal name="ZZZ_J4_INTERNAL"/>
<signal name="SIG$75"/>
<signal name="GND_2"/>
<signal name="GND_3"/>
<signal name="VBUS"/>
<signal name="SIG$79"/>
<signal name="SIG$81"/>
<signal name="COM"/>
<signal name="SIG$87"/>
<signal name="3"/>
<signal name="SIG$90"/>
<signal name="SIG$91"/>
<signal name="SIG$92"/>
<signal name="SIG$93"/>
<signal name="SIG$94"/>
<signal name="SIG$95"/>
<signal name="K"/>
<signal name="SIG$97"/>
<signal name="SIG$98"/>
<signal name="SIG$99"/>
<signal name="SIG$100"/>
<signal name="SIG$101"/>
<signal name="GND_4"/>
<signal name="SIG$103"/>
<signal name="SIG$104"/>
<signal name="SIG$105"/>
<signal name="SIG$106"/>
<signal name="SIG$107"/>
<signal name="SIG$108"/>
<signal name="SIG$109"/>
<signal name="SIG$111"/>
<signal name="SIG$113"/>
<signal name="V+"/>
<signal name="SIG$115"/>
<signal name="SIG$116"/>
<signal name="SIG$117"/>
<signal name="SIG$118"/>
<signal name="SIG$119"/>
<signal name="SIG$120"/>
<signal name="SIG$121"/>
<signal name="1">
<contactref element="U1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="SIG$124">
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SIG$125"/>
<signal name="SIG$126"/>
<signal name="SIG$127"/>
<signal name="5V">
<contactref element="U1" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="U3" pad="7"/>
<contactref element="R5" pad="2"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="SIG$129">
<contactref element="U2" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="D0"/>
<signal name="SIG$131"/>
<signal name="SIG$132">
<contactref element="U1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SIG$133">
<contactref element="U1" pad="5"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SIG$134"/>
<signal name="SIG$136"/>
<signal name="SIG$137"/>
<signal name="SIG$138">
<contactref element="U3" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SIG$139">
<contactref element="U3" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="SIG$140">
<contactref element="U1" pad="3"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="-">
<contactref element="U3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SIG$142"/>
<signal name="SIG$143">
<contactref element="C4" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="SIG$144"/>
<signal name="K_2">
<contactref element="D1" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="+VO"/>
<signal name="SIG$147">
<contactref element="R1" pad="2"/>
<contactref element="R9" pad="3"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="IN1">
<contactref element="U4" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="U4" pad="2"/>
</signal>
<signal name="V-"/>
<signal name="VCC"/>
</signals>
</board>
</drawing>
</eagle>
