|  |  |
| --- | --- |
| Arduino Nano/Mega/Uno | Sound Sensor |
| 5v | 5v |
| Gnd | Gnd |
| Analog Pin 0 | Output |

|  |  |
| --- | --- |
| Arduino Nano/Mega/Uno | Led 1,Led 2,Led3 |
| Digital pin 10 | Led 1 +ve with 200 ohm resistor |
| Digital pin 9 | Led 2 +ve with 200 ohm resistor |
| Digital pin 8 | Led 3 +ve with 200 ohm resistor |
| gnd | Gnd all Led;s together |