<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="62" y2="54" width="0" layer="20"/>
<wire x1="62" y1="54" x2="0" y2="54" width="0" layer="20"/>
<wire x1="0" y1="54" x2="0" y2="0" width="0" layer="20"/>
<hole x="3" y="3" drill="2.8"/>
<hole x="59" y="3" drill="2.8"/>
<hole x="59" y="51" drill="2.8"/>
<hole x="3" y="51" drill="2.8"/>
<text>MP26123/4 Li Battery Charger</text>
<text>MP26123/4 Li Battery Charger</text>
<text>J8</text>
<text>Batt+</text>
<text>Batt+</text>
<text>Batt-</text>
<text>Batt-</text>
<text>En</text>
<text>Load+</text>
<text>Load+</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>3.3VMP</text>
<text>PS_EN</text>
<text>PS_En</text>
<text>SR_Off</text>
<text>SR_On</text>
<text>CHGOK</text>
<text>Disable</text>
<text>NTC</text>
<text>VIN</text>
<text>github.com/thedalles77/Laptop-Battery-Charger</text>
<text>github.com/thedalles77/Laptop-Battery-Charger</text>
<text>3.3VAP</text>
<text>Gnd</text>
<text>Rev 1.1</text>
<text>Rev 1.1</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CAPC3225X280N">
<description>&lt;b&gt;1210/-&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CAPC3225X270N">
<description>&lt;b&gt;MK325(1210)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="DIOM7959X250N">
<description>&lt;b&gt;SMC&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="FUSC3216X105N">
<description>&lt;b&gt;0469005.WR&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="QFN65P400X400X100-17N">
<description>&lt;b&gt;QFN16 (4 x 4mm)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOIC127P600X175-8N">
<description>&lt;b&gt;SOIC8 CASE 751EB_&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="RESC6332X71N">
<description>&lt;b&gt;RESC6332X71N&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="0603_RESISTOR">
<packages>
<package name="0603_RESISTOR">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="DR73_NRS8030T">
<packages>
<package name="NRS8030">
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_5MM">
</package>
</packages>
</library>
<library name="AP7381">
<packages>
<package name="AP7381">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SamacSys_Parts" package="CAPC3225X280N" value="C1210C226K3PACTU">
<attribute name="DESCRIPTION" value="KEMET 1210 (3225M) 22uF Multilayer Ceramic Capacitor MLCC 25V dc +/-10% SMD C1210C226K3PACTU"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Kemet"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="C1210C226K3PACTU"/>
<attribute name="MOUSER_PART_NUMBER" value="80-C1210C226K3P"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/KEMET/C1210C226K3PACTU?qs=lm8WgJiVcEsXoa%2FG19fsAg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="1.0µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0805" value="1.0µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SamacSys_Parts" package="CAPC3225X270N" value="GMK325AB7106MM-T">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT 10uF 35V X7R +/-20% 1210 Gen Purp"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="TAIYO YUDEN"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GMK325AB7106MM-T"/>
<attribute name="MOUSER_PART_NUMBER" value="963-GMK325AB7106MM-T"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=963-GMK325AB7106MM-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SamacSys_Parts" package="CAPC3225X270N" value="GMK325AB7106MM-T">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT 10uF 35V X7R +/-20% 1210 Gen Purp"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="TAIYO YUDEN"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GMK325AB7106MM-T"/>
<attribute name="MOUSER_PART_NUMBER" value="963-GMK325AB7106MM-T"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=963-GMK325AB7106MM-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0805" value="1.0µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SamacSys_Parts" package="CAPC3225X280N" value="C1210C475K5RACTU">
<attribute name="DESCRIPTION" value="Capacitor 1210 4.7uF 50V Kemet 1210 C 4.7uF Ceramic Multilayer Capacitor, 50 V dc, +125C, X7R Dielectric, +/-10%"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Kemet"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="C1210C475K5RACTU"/>
<attribute name="MOUSER_PART_NUMBER" value="80-C1210C475K5R"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/KEMET/C1210C475K5RACTU?qs=dB0LedT%252BmmBpncka1nOCUg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.15µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="2200pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="2200pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SamacSys_Parts" package="DIOM7959X250N" value="B540C-13-F">
<attribute name="DESCRIPTION" value="Diodes Inc B540C-13-F, SMT Schottky Diode, 40V 5A, 2-Pin DO-214AB"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="B540C-13-F"/>
<attribute name="MOUSER_PART_NUMBER" value="621-B540C-F"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/B540C-13-F/?qs=v2dnQLbuoRZXHN%2FK4ft5%252Bg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="SamacSys_Parts" package="FUSC3216X105N" value="0469005.WR">
<attribute name="DESCRIPTION" value="LITTELFUSE - 0469005.WR - FUSE, SMD, 1206, SLOW BLOW, 5A"/>
<attribute name="HEIGHT" value="1.05mm"/>
<attribute name="MANUFACTURER_NAME" value="LITTELFUSE"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="0469005.WR"/>
<attribute name="MOUSER_PART_NUMBER" value="576-0469005.WR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Littelfuse/0469005WR?qs=fp%2Fo%2FcJ74ol%2F%2F%2FgXy9%2FuRQ%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SamacSys_Parts" package="QFN65P400X400X100-17N" value="MP26123DR-LF-Z">
<attribute name="DESCRIPTION" value="Battery Management 2A 24Vin 2-3 Cell Switching Charger"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Monolithic Power Systems (MPS)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MP26123DR-LF-Z"/>
<attribute name="MOUSER_PART_NUMBER" value="946-MP26123DRLFZ"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Monolithic-Power-Systems-MPS/MP26123DR-LF-Z?qs=ddTkeYFZflVgOJRHHyrLxQ%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="SamacSys_Parts" package="SOIC127P600X175-8N" value="FDS4435BZ">
<attribute name="DESCRIPTION" value="FDS4435BZ, P-channel MOSFET Transistor 8.8 A 30 V, 8-Pin SOIC"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="ON Semiconductor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FDS4435BZ"/>
<attribute name="MOUSER_PART_NUMBER" value="512-FDS4435BZ"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ON-Semiconductor-Fairchild/FDS4435BZ?qs=GXuM9q1TrDl7P7R1rhmrgw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="74xx-us" package="SO14" value="74132D">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="VIN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="NTC Sensor">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X02" value="Power Control">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X05" value="Battery Connections">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X02" value="3.3V MP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X02" value="PS Disable">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04" value="Power Supply Loads">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="0603_RESISTOR" package="0603_RESISTOR" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SamacSys_Parts" package="RESC6332X71N" value="WSL2512R2000FEA">
<attribute name="DESCRIPTION" value="RESISTOR, 2512 0.2 Ohm +/- 1.0 % 1 W"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Vishay"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="WSL2512R2000FEA"/>
<attribute name="MOUSER_PART_NUMBER" value="71-WSL2512R2000FEA"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=71-WSL2512R2000FEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="0603_RESISTOR" package="0603_RESISTOR" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="0603_RESISTOR" package="0603_RESISTOR" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="0603_RESISTOR" package="0603_RESISTOR" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="0603_RESISTOR" package="0603_RESISTOR" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="0603_RESISTOR" package="0603_RESISTOR" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="0603_RESISTOR" package="0603_RESISTOR" value="2.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="0603_RESISTOR" package="0603_RESISTOR" value="750">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="DR73_NRS8030T" package="NRS8030" value="4.7uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SamacSys_Parts" package="SOIC127P600X175-8N" value="FDS4435BZ">
<attribute name="DESCRIPTION" value="FDS4435BZ, P-channel MOSFET Transistor 8.8 A 30 V, 8-Pin SOIC"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="ON Semiconductor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FDS4435BZ"/>
<attribute name="MOUSER_PART_NUMBER" value="512-FDS4435BZ"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ON-Semiconductor-Fairchild/FDS4435BZ?qs=GXuM9q1TrDl7P7R1rhmrgw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="0603_RESISTOR" package="0603_RESISTOR" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="Pi Signals">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="oshw" package="OSHW_5MM" value=""/>
<element name="R5" library="0603_RESISTOR" package="0603_RESISTOR" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="AP7381" package="AP7381" value="AP7381-33Y-13">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0805" value="2.2µF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X02" value="3.3V AP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC4" pad="7"/>
<contactref element="C12" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="4"/>
<contactref element="C9" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="IC2" pad="12"/>
<contactref element="J1" pad="2"/>
<contactref element="J6" pad="4"/>
<contactref element="J6" pad="5"/>
<contactref element="R16" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="IC2" pad="17"/>
<contactref element="U1" pad="P$4"/>
<contactref element="U1" pad="P$3"/>
<contactref element="C17" pad="2"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="V3P3">
<contactref element="IC4" pad="14"/>
<contactref element="C13" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="U1" pad="P$1"/>
<contactref element="C17" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="VLOAD">
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="P$2"/>
</signal>
<signal name="INTERNAL_SW">
<contactref element="IC2" pad="15"/>
<contactref element="C5" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="CURRENT_SENSE_P">
<contactref element="IC2" pad="11"/>
<contactref element="R12" pad="1"/>
<contactref element="L1" pad="P$2"/>
</signal>
<signal name="ON_N">
<contactref element="IC4" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="TURN_OFF">
<contactref element="IC4" pad="10"/>
<contactref element="IC4" pad="9"/>
<contactref element="R13" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="TURN_OFF_N">
<contactref element="IC4" pad="8"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="CLR_N">
<contactref element="R14" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="Q">
<contactref element="IC4" pad="3"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="QBAR">
<contactref element="IC4" pad="2"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="BATTERY">
<contactref element="C12" pad="1"/>
<contactref element="IC2" pad="10"/>
<contactref element="J6" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="PS_DISABLE">
<contactref element="IC4" pad="11"/>
<contactref element="J8" pad="1"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="DISABLE">
<contactref element="R1" pad="2"/>
<contactref element="IC2" pad="6"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="BST">
<contactref element="IC2" pad="14"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="TMR">
<contactref element="C6" pad="1"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="COMPI">
<contactref element="IC2" pad="9"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R11" pad="1"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="C7" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="COMPV">
<contactref element="R10" pad="2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="CELLS">
<contactref element="IC2" pad="7"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="NTC">
<contactref element="IC2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="CHGOK">
<contactref element="IC2" pad="4"/>
<contactref element="R7" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="SYSTEM_PRESENT">
<contactref element="R16" pad="1"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="INPUT_GATE">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$3">
</signal>
<signal name="N$5">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="VCC">
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="FUSE_OUT">
<contactref element="F1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="5"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="MP3V3">
<contactref element="J7" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="R9" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
