<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="0" x2="54.61" y2="0" width="0.1524" layer="20"/>
<wire x1="54.61" y1="58.42" x2="5.08" y2="58.42" width="0.1524" layer="20"/>
<wire x1="0" y1="53.34" x2="0" y2="5.08" width="0.1524" layer="20"/>
<wire x1="59.69" y1="53.34" x2="59.69" y2="5.08" width="0.1524" layer="20"/>
<wire x1="0" y1="53.34" x2="5.08" y2="58.42" width="0.1524" layer="20" curve="-90"/>
<wire x1="59.69" y1="53.34" x2="54.61" y2="58.42" width="0.1524" layer="20" curve="90"/>
<wire x1="59.69" y1="5.08" x2="54.61" y2="0" width="0.1524" layer="20" curve="-90"/>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0.1524" layer="20" curve="90"/>
<text>SWCLK</text>
<text>SWDIO</text>
<text>5V</text>
<text>GND</text>
<text>3V3</text>
<text>NRST</text>
<text>SWO</text>
<text>GND</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>3V3</text>
<text>RGB Mode</text>
<text>Reset</text>
<text>Osu! Keypad</text>
<text>V1.1</text>
<text>2/20/2021</text>
<text>designed by Xieshi Zhang</text>
<text>BT0</text>
<text>BT1</text>
<text>instructables.com/member/CrazyBlackStone</text>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="bt_diode">
<description>Diodes, rectifiers, regulators</description>
<packages>
<package name="SOD123FL">
<description>SOD-123. Should fit SOD-123, SOD-123FL, and others.</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="micro-stm_v3">
<description>&lt;b&gt;ARM 32-bit Cortex™ MCUs&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by jb@jenszuhause.de&lt;/author&gt;&lt;p&gt;
&lt;b&gt;You are using this libary by your own risk.&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Make sure to check everything well due to this libary before using it.&lt;/b&gt;</description>
<packages>
<package name="LQFP48">
<description>&lt;b&gt;LQFP48&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 48-pin low-profile quad flat package</description>
</package>
</packages>
</library>
<library name="USB3090-XX-X_REVE">
<packages>
<package name="GCT_USB3090-XX-X_REVE">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="0ZCH0050FF2G">
<packages>
<package name="RESC3225X75N">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="1825910-6">
<packages>
<package name="SW_1825910-6-4">
</package>
</packages>
</library>
<library name="Keyboard">
<description>Keyboard Keyswitch PCB footprints for MX and Alps switches.</description>
<packages>
<package name="MXHSPCB-1U">
<description>Keyboard switch package!</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SunLED - XZMDKCBDDG45S-9">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="SUNLED_XZMDKCBDDG45S-9_0">
<description>Red, Green, Blue (RGB) 630nm Red, 525nm Green, 465nm Blue LED Indication - Discrete 1.95V Red, 3.3V Green, 3.3V Blue 4-SMD, Gull Wing</description>
</package>
</packages>
</library>
<library name="RK7002BMT116">
<packages>
<package name="TRANS_RK7002BMHZG_ROM-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0805" value="1u">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805" value="4.7u">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="20p">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="20p">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0805" value="100n">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="bt_diode" package="SOD123FL" value="DIODE_SOD123FL">
<attribute name="VALUE"/>
</element>
<element name="H2" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPULARITY" value="7"/>
</element>
<element name="H3" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPULARITY" value="7"/>
</element>
<element name="H4" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPULARITY" value="7"/>
</element>
<element name="IC1" library="micro-stm_v3" package="LQFP48" value="STM32F103C8T">
<attribute name="VALUE"/>
</element>
<element name="J1" library="USB3090-XX-X_REVE" package="GCT_USB3090-XX-X_REVE" value="USB3090-XX-X_REVE">
<attribute name="AVAILABILITY" value="Warning"/>
<attribute name="DESCRIPTION" value=" USB - micro AB USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle; Through Hole, 2.35mm profile, 5 Pins, Horizontal, Bottom mount "/>
<attribute name="MF" value="Global Connector Technology"/>
<attribute name="MP" value="USB3090-30-A"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/USB3090-30-A/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X04/90" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="9"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X04/90" value="">
<attribute name="POPULARITY" value="9"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X03/90" value="">
<attribute name="POPULARITY" value="17"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="crystal" package="HC49/S" value="8MHZ">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="49"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="0ZCH0050FF2G" package="RESC3225X75N" value="0ZCH0050FF2G">
<attribute name="DESCRIPTION" value=" 1210 SMT PPTC | 0.50 Ih | 16V "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="507-1786-1-ND"/>
<attribute name="MF" value="Bel Fuse"/>
<attribute name="MP" value="0ZCH0050FF2G"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="1210 Bel Fuse"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/0ZCH0050FF2G/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="68">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="1k5">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="68">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0805" value="1k5">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="68">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="1k5">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="1k5">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="10k">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="10k">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="68">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="1k5">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="1825910-6" package="SW_1825910-6-4" value="1825910-6">
<attribute name="COMMENT" value="1825910-6"/>
<attribute name="CONFIGURATION_POLE-THROW" value="Single Pole - Single Throw"/>
<attribute name="CONTACT_CURRENT_RATING" value="50 mA"/>
<attribute name="DESCRIPTION" value=" Switch Push Button OFF (ON) SPST Round Button 0.05A 24VDC Momentary Contact PC Pins Thru-Hole "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="450-1650-ND"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="1825910-6"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/1825910-6/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="H5" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPULARITY" value="7"/>
</element>
<element name="R13" library="rcl" package="R0805" value="10k">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0805" value="10k">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="10k">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value="100n">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0805" value="1u">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value="100n">
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="SOT223" value="MCP1703DB">
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="10k">
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U"/>
<element name="U$6" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U"/>
<element name="U$7" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U"/>
<element name="U$8" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U"/>
<element name="D2" library="SunLED - XZMDKCBDDG45S-9" package="SUNLED_XZMDKCBDDG45S-9_0" value="SUNLED_XZMDKCBDDG45S-9SUNLED_XZMDKCBDDG45S-9_0_0">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="Red, Blue, Green"/>
<attribute name="DATASHEET" value="http://www.sunledusa.com/products/spec/XZMDKCBDDG45S-9.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="LED RGB CLEAR 4PLCC SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1497-1257-1-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="20mA"/>
<attribute name="FORWARD_VOLTAGE" value="1.95/3.3/3.3V"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Straight"/>
<attribute name="LUMINOUS_INTENSITY" value="108/98/497mcd"/>
<attribute name="MF" value="SunLED"/>
<attribute name="MFG_PACKAGE_IDENT" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUNTING_TYPE" value="Surface Mount, Bottom Entry"/>
<attribute name="MPN" value="XZMDKCBDDG45S-9"/>
<attribute name="PACKAGE" value="SMD4"/>
<attribute name="PEAK_EMMISION_WAVELENGTH" value="645/460/515nm"/>
<attribute name="POWER_DISSIPATION" value="75/120/123mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
<attribute name="VIEWING_ANGLE" value="120°"/>
<attribute name="WAVELENGTH" value="630/465/525nm"/>
</element>
<element name="D3" library="SunLED - XZMDKCBDDG45S-9" package="SUNLED_XZMDKCBDDG45S-9_0" value="SUNLED_XZMDKCBDDG45S-9SUNLED_XZMDKCBDDG45S-9_0_0">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="Red, Blue, Green"/>
<attribute name="DATASHEET" value="http://www.sunledusa.com/products/spec/XZMDKCBDDG45S-9.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="LED RGB CLEAR 4PLCC SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1497-1257-1-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="20mA"/>
<attribute name="FORWARD_VOLTAGE" value="1.95/3.3/3.3V"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Straight"/>
<attribute name="LUMINOUS_INTENSITY" value="108/98/497mcd"/>
<attribute name="MF" value="SunLED"/>
<attribute name="MFG_PACKAGE_IDENT" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUNTING_TYPE" value="Surface Mount, Bottom Entry"/>
<attribute name="MPN" value="XZMDKCBDDG45S-9"/>
<attribute name="PACKAGE" value="SMD4"/>
<attribute name="PEAK_EMMISION_WAVELENGTH" value="645/460/515nm"/>
<attribute name="POWER_DISSIPATION" value="75/120/123mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
<attribute name="VIEWING_ANGLE" value="120°"/>
<attribute name="WAVELENGTH" value="630/465/525nm"/>
</element>
<element name="D4" library="SunLED - XZMDKCBDDG45S-9" package="SUNLED_XZMDKCBDDG45S-9_0" value="SUNLED_XZMDKCBDDG45S-9SUNLED_XZMDKCBDDG45S-9_0_0">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="Red, Blue, Green"/>
<attribute name="DATASHEET" value="http://www.sunledusa.com/products/spec/XZMDKCBDDG45S-9.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="LED RGB CLEAR 4PLCC SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1497-1257-1-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="20mA"/>
<attribute name="FORWARD_VOLTAGE" value="1.95/3.3/3.3V"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Straight"/>
<attribute name="LUMINOUS_INTENSITY" value="108/98/497mcd"/>
<attribute name="MF" value="SunLED"/>
<attribute name="MFG_PACKAGE_IDENT" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUNTING_TYPE" value="Surface Mount, Bottom Entry"/>
<attribute name="MPN" value="XZMDKCBDDG45S-9"/>
<attribute name="PACKAGE" value="SMD4"/>
<attribute name="PEAK_EMMISION_WAVELENGTH" value="645/460/515nm"/>
<attribute name="POWER_DISSIPATION" value="75/120/123mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
<attribute name="VIEWING_ANGLE" value="120°"/>
<attribute name="WAVELENGTH" value="630/465/525nm"/>
</element>
<element name="D5" library="SunLED - XZMDKCBDDG45S-9" package="SUNLED_XZMDKCBDDG45S-9_0" value="SUNLED_XZMDKCBDDG45S-9SUNLED_XZMDKCBDDG45S-9_0_0">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="Red, Blue, Green"/>
<attribute name="DATASHEET" value="http://www.sunledusa.com/products/spec/XZMDKCBDDG45S-9.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="LED RGB CLEAR 4PLCC SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1497-1257-1-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="20mA"/>
<attribute name="FORWARD_VOLTAGE" value="1.95/3.3/3.3V"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Straight"/>
<attribute name="LUMINOUS_INTENSITY" value="108/98/497mcd"/>
<attribute name="MF" value="SunLED"/>
<attribute name="MFG_PACKAGE_IDENT" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUNTING_TYPE" value="Surface Mount, Bottom Entry"/>
<attribute name="MPN" value="XZMDKCBDDG45S-9"/>
<attribute name="PACKAGE" value="SMD4"/>
<attribute name="PEAK_EMMISION_WAVELENGTH" value="645/460/515nm"/>
<attribute name="POWER_DISSIPATION" value="75/120/123mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
<attribute name="VIEWING_ANGLE" value="120°"/>
<attribute name="WAVELENGTH" value="630/465/525nm"/>
</element>
<element name="SW2" library="1825910-6" package="SW_1825910-6-4" value="1825910-6">
<attribute name="COMMENT" value="1825910-6"/>
<attribute name="CONFIGURATION_POLE-THROW" value="Single Pole - Single Throw"/>
<attribute name="CONTACT_CURRENT_RATING" value="50 mA"/>
<attribute name="DESCRIPTION" value=" Switch Push Button OFF (ON) SPST Round Button 0.05A 24VDC Momentary Contact PC Pins Thru-Hole "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="450-1650-ND"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="1825910-6"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/1825910-6/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="RK7002BMT116" package="TRANS_RK7002BMHZG_ROM-M" value="RK7002BMT116TRANS_RK7002BMHZG_ROM-M">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RK7002BMT116"/>
<attribute name="SOURCELIBRARY" value="Rohm_2019-09-23"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
<element name="Q3" library="RK7002BMT116" package="TRANS_RK7002BMHZG_ROM-M" value="RK7002BMT116TRANS_RK7002BMHZG_ROM-M">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RK7002BMT116"/>
<attribute name="SOURCELIBRARY" value="Rohm_2019-09-23"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
<element name="Q1" library="RK7002BMT116" package="TRANS_RK7002BMHZG_ROM-M" value="RK7002BMT116TRANS_RK7002BMHZG_ROM-M">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RK7002BMT116"/>
<attribute name="SOURCELIBRARY" value="Rohm_2019-09-23"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
</elements>
<signals>
<signal name="SHIELD">
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="SWCLK">
<contactref element="IC1" pad="37"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SWDIO">
<contactref element="IC1" pad="34"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="SW1" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC1" pad="35"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="NRST">
<contactref element="IC1" pad="7"/>
<contactref element="JP2" pad="4"/>
<contactref element="SW1" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="TRACESWO">
<contactref element="IC1" pad="39"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="+3V3">
<contactref element="R2" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="48"/>
<contactref element="IC1" pad="36"/>
<contactref element="IC1" pad="24"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="9"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="SJ2" pad="2"/>
<contactref element="U$5" pad="MX2"/>
<contactref element="U$6" pad="MX2"/>
<contactref element="U$7" pad="MX2"/>
<contactref element="U$8" pad="MX2"/>
<contactref element="D4" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="5"/>
<contactref element="X1" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="6"/>
<contactref element="X1" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="BOOT0">
<contactref element="R3" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="IC1" pad="44"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="BOOT1">
<contactref element="IC1" pad="20"/>
<contactref element="JP2" pad="2"/>
<contactref element="SJ2" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="GATER">
<contactref element="IC1" pad="11"/>
<contactref element="R13" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GATEG">
<contactref element="IC1" pad="12"/>
<contactref element="R14" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="GATEB">
<contactref element="IC1" pad="13"/>
<contactref element="R15" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="G">
<contactref element="D2" pad="4"/>
<contactref element="D4" pad="4"/>
<contactref element="D3" pad="4"/>
<contactref element="D5" pad="4"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="B">
<contactref element="D2" pad="3"/>
<contactref element="D4" pad="3"/>
<contactref element="D3" pad="3"/>
<contactref element="D5" pad="3"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="R">
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="SW1">
<contactref element="IC1" pad="14"/>
<contactref element="R5" pad="1"/>
<contactref element="U$5" pad="MX1"/>
</signal>
<signal name="SW2">
<contactref element="IC1" pad="15"/>
<contactref element="R6" pad="1"/>
<contactref element="U$6" pad="MX1"/>
</signal>
<signal name="SW3">
<contactref element="IC1" pad="16"/>
<contactref element="R7" pad="1"/>
<contactref element="U$7" pad="MX1"/>
</signal>
<signal name="SW4">
<contactref element="IC1" pad="17"/>
<contactref element="R8" pad="1"/>
<contactref element="U$8" pad="MX1"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="D4" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D5" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="MODE">
<contactref element="IC1" pad="18"/>
<contactref element="SW2" pad="3"/>
<contactref element="SW2" pad="4"/>
</signal>
<signal name="D_P">
<contactref element="IC1" pad="33"/>
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D_N">
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="32"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
